In the case of a seeker measuring the los angle directly in one dimension.

The model for luenberger observer:

Assumptions:

Non maneuvering target, path angles near the los.

Reference state